
Modified Short Course
Chassis
· 1/10 2wd Short Course Truck
· Wheelbase 320-335mm
Motor/ESC
· Open Brushless -or- Brushed ESC
· Open Brushless -or- Brushed Motor
Battery
· s Lithium Battery
· Charged to 8.44v Max
Body
· Full fender truck
· Must completely cover tires when viewed from above
Tires
· Any 2.2”x3.0” Rubber SCT Size Tire
Transmission
· Single Speed Transmissions Only
· Gear or Ball Diff Permitted
Weight
· Minimum 2098g


**Chassis Protectors Required for Flat Bottom Chassis**
**RPM80902 Required for Slash Chassis**
**Help Preserve the Carpet!!**

**Please refer to Roar Rule Book Section 1.3 for specifics**
Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

