
Stock Slash
Chassis
· 1/10 2wd Slash Chassis
· Stock High CG Chassis Only
· Must run RPM Bumper Mount (RPM80902)
· ALL PARTS MUST BE RUN IN THEIR ORIGINAL INTENDED LOCATION
Motor/ESC
· Titan 12t & XL5
· BL-2s Motor Combo (#3382)
· Fans NOT permitted for use on Motor or ESC
Battery
· 2s Lithium Polymer Battery
· Charged to 8.44v Max
· 6-7 Cell NiMh
Body
· Full fender truck
· Must completely cover tires when views from above
Shocks
· Stock Ultra Shocks Only
· Aluminum Traxxas Caps Permitted
· Can use any Traxxas Progressive Rate Spring made for Ultra Shocks
· Can use any weight oil
· Cannot use any shock limiters
Tires
· Traxxas Khumo Tires 
· Traxxas BFGoodrich Tires
· Traxxas SCT Tires
· Can use S1 Compound Tires
· Must run front on front and rear on rear
· CA Glue permitted for use only on the sidewalls - never on the tread
Transmission
· Stock Case only (Magnum 272R NOT Permitted)
· Stock transmission gears only (Aluminum Idler Permitted)
· Stock Diff only
· No lockout
· Can use any oil/grease
Upgraded Parts
· Any RPM upgrade that DOES NOT change the performance or geometry of the vehicle (i.e. Trans. Case)
· Only Stock Traxxas & RPM Brand parts permitted
· Stock Hinge Pins only
· Traxxas Driveshafts Only (1951, 6852X, 6852A) 
· Rear RPM Bumper Mount (RPM80902) REQUIRED
· STRC Parts are NOT legal
· No Aluminum Parts Permitted (Except otherwise specified in previous rules)

**RPM80902 REQUIRED**
**Help Preserve the Carpet - CHECK ALL SCREWS**
Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

