
1/12 LMP
Chassis
· 1/12 scale 2wd
· 3mm Minimum Ride Height 
Motor/ESC
· ROAR approved 17.5T Brushless
· “Blinky” Mode ESC (No Boost / Turbo / Internal Timing} 
Battery
· Any ROAR Approved 1s Lipo
· Charged to 4.2V Maximum
Body
· ROAR approved LMP / GTP / WSC style
Tires
· Purple/Blue Striped foam only
Transmission
· Single 1-piece drive axle
· No independent rear suspension
Weight
· 730 gr

Additional rules may be listed at ROAR, page 51. Racer is responsible for their car being legal within all these rules
Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

