
25.5 TC
Chassis
· 4wd Touring Car, independent front and rear suspension.
Motor/ESC
· ROAR approved 25.5T motor, ESC in Sportsman / Blinky mode.
Battery
· ROAR approved 2S LiPo charged to 8.4V maximum
Body
· Any ROAR approved TC body
Tires
· Gravity RC GRC132: Type C Touring Spec Tire only
Transmission
· Single Speed, 4wd
Weight
· 1320 grams
Ride Height
· 5mm


https://www.roarracing.com/downloads/ROAR_Rule_Book.pdf

Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

