
F1
Chassis
· 1/10 scale 2wd
· Chassis must be a commercially available dedicated F1 chassis. No 1/12 or 1/10 “pan car” conversions
· All suspension mount points must fit within the body
· Car must appear within the “spirit” of actual F1 cars
· 4 tires only
· 190mm maximum width
· 3mm Minimum Ride Height
Motor/ESC
· ROAR approved 25.5T Brushless
· “Blinky” Mode ESC (No Boost / Turbo / Internal Timing} 
Battery
· Any ROAR Approved 2s Lipo
· Charged to 8.4V Maximum
Body
· Bodies must be modeled to resemble cars raced from 2008 to present
· Cars must race with front and rear wings.
· lexan wings are not permitted
Tires
· Any commercially available rubber F1 tire, mounted on a hex-style wheel
Transmission
· Single 1-piece drive axle
· No independent rear suspension
Weight
· 1020 gr

Additional rules may be listed at HERE. Racer is responsible for their car being legal within all these rules



Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

