
Figure 8
Chassis
· Traxxas Slash 2WD Chassis
· Stock High CG or Low CG Chassis allowed
· No modifying chassis
· 8mm Minimum Ride Height 
· Adding weight is permitted inside pan only
· All parts must be run in their original location
Motor/ESC
· Any brushless combo within a 10.5T or 4000KV Limit
Steering/Servo
· Any standard 1/10 Scale Servo
· Recommended to run Servo Saver
· Stock, Aluminum or 4x4 rack permitted
Battery
· Any ROAR Approved 2s Lipo
· Charged to 8.44V Maximum
· Shorty or Full Size pack permitted
Body
· Any body made for SCT Chassis
· Handmade Late Model Bodies permitted
· Top of wing cannot be higher than 8” from ground when installed
· Lexan bodies only
· MAKE SURE ALL CORNERS/EDGES ARE WELL-ROUNDED - RACE DIRECTOR MAY REQUIRE ADDITIONAL TRIMMING
Bumper
· Stock or RPM front/rear permitted
· No aluminum bumpers
· MUST run Front and Rear Bumper
· Nerf Bars not required
· Rear RPM Bumper Mount REQUIRED
Tires
· Any 2.2” Stadium Truck Slick Tire
· Any offset of 2.2” wheels
· Stock Traxxas SCT Tires permitted
Transmission
· Stock, Proline, or Magnum 272R only
· No Mid-Motor Conversion permitted
· Can use Hot Racing Sealed Diff Case
· Can use any oil/grease
Shocks
· Traxxas Shocks
· Ultra, Big Bore, GTR
· Proline Shocks for Slash
· Powerstroke Shock
· Must use Springs designed for your shock
· Can run any internal limiter
· External Limiters not permitted
· Can run any fluid
Upgraded Parts
· Any RPM or Traxxas Brand upgrade made for Slash
· Any aluminum upgrade except for:
· Arms, Chassis, Bumpers
· All parts MUST be designed for a Slash
· Steel CVD Permitted
· Rear RPM Bumper Mount (RPM80902) REQUIRED
· Any STRC Part is legal, except conflicting with previous rule

Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

