
Slash Street Stock
1.0.0 Chassis
· 1.1.0 	Traxxas Slash 2WD Kit
· 1.2.0 	Stock High CG or Low CG Chassis permitted
· 1.3.0 	No modifying chassis
· 1.4.0	8mm Minimum Ride Height
· 1.5.0 	Adding weight is permitted (inside pan only)
· 1.6.0 	All parts must be run in their original intended location
2.0.0 Motor/ESC
· 2.1.0 	Traxxas Titan 12t & XL5 Combo
· 2.2.0 	Traxxas BL-2s Combo (#3382)
· 2.3.0 	Fans NOT Permitted for use on Motor or ESC
3.0.0 Steering/Servo
· 3.1.0 	Any standard 1/10 Scale Servo
· 3.2.0 	Stock steering rack or 4x4 steering rack only
· 3.3.0 	Any Servo Horn or Servo Saver
4.0.0 Body
· 4.1.0	 Any stock car style body within the spirit of the class
· 4.1.1	 Excluding Late Model Body, Truck Bodies, GT Style Bodies
· 4.2.0 	Body must be between 11 and 12 inches wide
· 4.2.1	 Tires CANNOT stick out more than ½” past fenders
· 4.2.2	 Fenders can be cut; however bodies cannot be cut into hood
· 4.3.0	 Inquire at track for approval
5.0.0 Tires/Wheels  	
· 5.1.0	 Any 2.2” Stadium Truck Slick Rubber Tire
· 5.1.1	Must be a commercially available slick - cannot grind tires down to slicks
· 5.2.0	 Any offset of 2.2” Stadium Truck Wheels (50mm +/- 3mm Width)
· 5.2.1	 Refer to 4.2.1 regarding offset limits
6.0.0 Bumper
· 6.1.0	 Stock or RPM front/rear permitted
· 6.2.0	 No aluminum bumpers
· 6.3.0	 MUST run Front and Rear Bumper
· 6.4.0 	Nerf Bars not required
· 6.5.0	 Rear RPM Bumper Mount REQUIRED
7.0.0 Transmission
· 7.1.0	 Stock Case only (Magnum 272R NOT Permitted)
· 7.2.0	 Stock transmission gears only (Aluminum Idler Permitted)
· 7.3.0 	Stock Diff only
· 7.3.1	 No lockout
· 7.4.0 	Can use any oil/grease
· 7.5.0         Slipper Eliminators are not legal 
8.0.0 Shocks
· 8.1.0 	Stock Ultra Shocks only
· 8.1.1	 No aluminum (except caps), no titanium
· 8.1.2 	Any internal limiter allowed
· 8.1.3	 External Limiters not permitted
· 8.2.0	 Must use any Traxxas Progressive Rate Spring
9.0.0 Upgraded Parts
· 9.1.0 	 Any RPM upgrade that DOES NOT change the performance or geometry of the vehicle (i.e. Trans. Case)
· 9.2.0	 Only Stock Traxxas & RPM Brand parts permitted
· 9.3.0	 Stock Hinge Pins only
· 9.4.0	 Traxxas Driveshafts Only (1951, 6852X, 6852A) 
· 9.5.0	 Rear RPM Bumper Mount (RPM80902) REQUIRED
· 9.6.0	 STRC Parts are NOT legal
· 9.7.0	 No Aluminum Parts Permitted (Except otherwise specified in previous rules)
10.0.0 Battery
· 10.1.0	 Any ROAR Approved 2s Lipo
· 10.1.1	 Charged to 8.44V Maximum
· 10.2.0	 Battery must be run in original intended location
Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**
