

Sportsman RTT General Rules
Chassis
· 1/10 Pan Car / Straight axle chassis, “SS” style, with tires that fit inside body.
· ALL Chassis MUST be a mass manufactured chassis
· ABSOLUTELY NO PROTOTYPE CHASSIS / ONE-OFF CHASSIS
· This would include any chassis NOT mass manufactured and/or NOT available to general public
Motor
· Gravity 21.5T 45* TOUR Motor (GRC2010) only.
· Security Seal MUST remain intact
ESC
· ROAR approved 1S ESC set to Sportsman (blinky) mode (i.e. no timing boost, cheat modes,etc) at all times.
Battery
· Protek 3.8v 8800mah 130C (PTK-5105-22) -OR-
· Gens Ace 3.8v 8000mah 130C (GEA80001S13D5) ONLY
Body
· Protoform 1/10 ORT truck body (PRM122721) only
Tires
· CRC GTR rubber tires (CLN2314) only
Transmission
· Direct drive, single axle rear with a ball differential only No spools allowed.
Weight
· 39 oz / 1106 gr minimum
Ride Height
· 5mm

Racer is responsible for their car being legal within all these rules

More Specific rules listed here: TOUR Rules narrowed to RTT



Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

