
USAC Sprint
1.0.0 Chassis
· 1.1.0 	Traxxas Slash 2WD Chassis Only
· 1.2.0 	Low CG Chassis only 
· 1.3.0 	No modifying chassis pan
· 1.4.0 	8mm Minimum Ride Height 
· 1.5.0 	Adding weight is permitted inside pan only
· 1.6.0 	All parts must be run in their original location
2.0.0 Motor/ESC
· 2.1.0	Stock Titan 12T & XL5 ESC 
· 2.2.0	Hobbywing 13.5T Justock Motor & Justock ESC
· 2.2.1	PULL THE MOTOR OUT OF THE BOX AND RUN IT
· 2.2.2	ANY DISMANTLING OR MODIFICATION OF MOTOR IS CONSIDERED ILLEGAL
· 2.3.0	Traxxas BL-2s Motor Combo (3382)
3.0.0 Steering/Servo
· 3.1.0	Any standard 1/10 Scale Servo
· 3.2.0	Recommended to run Servo Saver
· 3.3.0	Stock, Aluminum or 4x4 rack permitted
4.0.0 Battery
· 4.1.0	Any ROAR Approved 2s Lipo
· 4.1.1	Charged to 8.44V Maximum
· 4.2.0	Shorty or Full Size pack permitted
5.0.0 Body
· 5.1.0	McAllister Mercer Sprint Body only
· 5.2.0	Track official may deny use of track for bodies with chipping paint
6.0.0 Bumper
· 6.1.0	Stock or RPM front/rear permitted
· 6.2.0	No aluminum bumpers
· 6.3.0	MUST run Front and Rear Bumper
· 6.4.0	Nerf Bars not required
· 6.5.0	Rear RPM Bumper Mount REQUIRED
7.0.0 Tires
· 7.1.0	Must run any 2.2” Stadium Truck Slick Tire on rear only, with 2.2” Stadium Truck Wheel
· 7.2.0	Must run any 2.2” Buggy rear slick tire on front only, with 2.2” Buggy Rear Wheel
8.0.0 Transmission
· 8.1.0	Stock Case or RPM
· 8.2.0	Stock Traxxas  transmission gears only (Aluminum Idler Permitted)
· 8.3.0	No Mid Motor Conversion Permitted
· 8.4.0	Can use Hot Racing Sealed Diff Case
· 8.5.0	Can use any oil/grease
9.0.0 Shocks
· 9.1.0	Must be Traxxas Ultra Shocks
· 9.1.1	Titanium shafts permitted
· 9.1.2	Aluminum caps permitted
· 9.2.0	Must use Traxxas Springs designed for your shock
· 9.3.0	Can run any internal limiter
· 9.3.1	External Limiters not permitted
· 9.4.0	Can run any fluid
10.0.0 Upgraded Parts
· 10.1.0	Any RPM upgrade made for Slash
· 10.2.0	Traxxas Driveshafts Only (1951, 6852X, 6852A) 
· 10.3.0	Any aluminum upgrade except for:
· 10.3.1	Bulkhead, Arms, Chassis, Shock Towers, Bumper
· 10.4.0	All parts MUST be designed for a Slash
· 10.5.0	STRC Hinge pins permitted

Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
Indy RC will confiscate ANY motor found to be illegal used in USAC
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**
