
Stock Buggy (17.5)
Chassis
· 1/10 2wd Buggy
Motor/ESC
· Roar Approved 17.5T Motor
· Roar Approved ESC
· Must be run in “Blinky” Mode
Battery
· Roar Approved 2s Lithium Battery
· Charged to 8.44v Max
Body
· Buggy or other off-road style body that resembles an actual off- road racing non-truck type vehicle
Tires
· Any 2.2” Rubber Buggy Size Tire
Transmission
· Single Speed Transmissions Only
· Gear or Ball Diff Permitted
Weight
· Minimum 1474g 



**Shock Tower Guards and Chassis Protectors Required**
**Help Preserve the Carpet - CHECK YOUR SCREWS**

**Please refer to Roar Rule Book Section 1.1 for specifics**


Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

