
Stadium Truck
Chassis
· 1/10 2wd Stadium Truck
· Wheelbase 229-292mm
Motor/ESC
· Open Brushless -or- Brushed ESC
· Open Brushless -or- Brushed Motor
Battery
· 2s Lithium Battery
· Charged to 8.44v Max
Body
· Off-road Truck style body only
Tires
· Any 2.2” Rubber Stadium Truck Size Tire
· Min Diameter - 91.5mm
· Max Width - 54mm
Transmission
· Single Speed Transmissions Only
· Gear or Ball Diff Permitted
Weight
· Minimum 1701g 

**Please refer to Roar Rule Book Section 1.2 for specifics**
Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

