
GT12
Chassis
· 1/12 scale 2wd
· 3mm Minimum Ride Height 
Motor/ESC
· Gravity RC USGT 21.5t Spec Motor (GRC2000)
· “Blinky” Mode ESC (No Boost / Turbo / Internal Timing} 
· 
Battery
· Any ROAR Approved 1s Lipo
· Charged to 4.2V Maximum
Body
· “GT” style bodies only
· Minimum Weight Painted - 45g
· If under, race director will add tape to the TOP of the body to bring it up to weight
· No LMP / GTP / WSC style bodies permitted
Tires
· GRC TYPE12  Rubber tires only
Transmission
· Single 1-piece drive axle
· No independent rear suspension
Weight
· 750 gr


Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

