
1/12 AWD Losi Nascar

· STOCK RADIO MUST BE USED
· STOCK TIRES MUST BE USED
· TIRE DOPE MAY BE USED
· CA MAY BE USED ON THE TIRE SIDEWALLS
· SHOCK OIL MAY BE CHANGED
· NO HOP-UP PARTS ALLOWED
· THE CAR MUST RUN WITH ALL PARTS IN THEIR ORIGINAL POSITION.
· NO MODIFICATIONS ARE ALLOWED TO THE CAR.
· RACE DIRECTOR MAY DISQUALIFY ANY CAR THEY FEEL IS “OUTSIDE” THE SPIRIT OF THE RULES
· OVERALL WEIGHT MINIMUM:
· MUST USE LOSI NASCAR BODY 
· LOS-1917; LOS-1918; LOS-1938
· BODY WEIGHT MINIMUM:100 grams


THIS IS A TOTAL BOX STOCK CLASS - NO ALTERATIONS OR MODIFICATIONS OF ANY KIND ARE PERMITTED




Make sure car is free of any debris/sharp edges 
No protruding screws on underside of chassis
Indy RC reserves the right to do random techs on any chassis at any point
**IF IT IS NOT ADDRESSED, DO NOT DO IT UNTIL IT IS APPROVED**

